# GPIO Functions - GrovePi Documentation
Python documentation for the GrovePi
Author: DexterInd Team

Skip to content


# API - GPIO Functions

In this section the Python API reference for GPIO functions is described. This library is supported on both major versions of Python: 2.x and 3.x.

IMPORTANT

This library and the other ones too are not thread-safe. You cannot call the GrovePi from multiple threads or processes as that will put the GrovePi into a broken state.

In case you need to reset the GrovePi from your Raspberry Pi, check this section.

The functions don't verify if the input parameters are valid and therefore the parameters have to be verified/validated before that. Calling a function with improper parameters can result in an undefined behavior for the GrovePi.

## `grovepi.digitalRead(pin)`

Reads whether a port's input is set high or low on the GrovePi.

Parameters

- `pin {Integer}` a number to identify the port (D2-D8) from which to do the reading

Returns: `0` or `1` depending on the input value

## `grovepi.digitalWrite(pin, value)`

Sets the output value to either `0` or `1` to a digital port on the GrovePi.

Parameters

- `pin {Integer}` a number to identify the port (D2-D8) to which to do the writing
- `value {Integer}` either `0` for 0 volts or `1` for maximum output voltage (usually 5 volts)

Returns: `1` all the time

## `grovepi.analogRead(pin)`

Detect an input voltage as a value from a given port on the GrovePi.

Parameters

- `pin {Integer}` a number to identify the port (A0-A2) from which to do the reading

Returns: a 10-bit `{Integer}` number that maps to the input voltage on the port

## `grovepi.analogWrite(pin, value)`

Set an output voltage on a PWM-enabled port by mapping the value to the desired voltage on the GrovePi.

Parameters

- `pin {Integer}` a number to identify the port (ports 3, 5, 6, 9) to which to do the writing
- `value {Integer}` an 8-bit number that maps from 0V to the referenced voltage of the GrovePi (5V)

Returns: `1` all the time

## `grovepi.pinMode(pin, mode)`

Sets a port to be either an OUTPUT or an INPUT port on the GrovePi.

Parameters

- `pin {Integer}` a number to identify the port (D2-D8) to which to do the change
- `mode {String}` `"OUTPUT"` for writing values or `"INPUT"` for reading

Returns: `1` all the time